* some of the pinouts don’t seem to work properly when used with the Python Adafruit library statements

Functional GPIO Pinouts

| P9\_27 | P9\_23 | P9\_26 | P9\_16 | P9\_12 | P9\_13 |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| P8\_26 | P8\_14 | P8\_11 | P8\_15 | P8\_9 | P8\_10 | P8\_13 | P8\_12 |
| P8\_16 |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |